**DOUBLE COLUMN GRINDING MACHINE**

Maker : ASCHESLEBEN/Germany

Type : SZ 10-10-03

New in : 1991

**Specifications:**

max. grinding width 1000 mm

max. grinding lenth 3000 mm

max. grinding height 1000 mm

distance betw. column 1500 mm

speed - table 1..50 m/min

total power 121 kW

weight of the machine 55 to

dimension of the machine 8.5 x 4.8 x 4.0 mm

electrics 380/50 V/Hz

**Accessories/Features:**

1.Universal Grinding Head, Type: UNI 7/1

- Power 7 kW

- Swivability +/- 90 deg.

- Vert. Adjustment 600 mm

2. Vertical Grinding Head, Type: USS 22/1

- Power 15 kW

- Vertical Travel 250 mm

**Price** :

**Delivery**: Immediately